scattering measurement with flashers EDML dust record Hole 66 dust log average dust log all scaled to location of hole 50

depth Μ m Ν dust Μ a.u. Ν

0 50 100 150 200 250 300 350 400 450 500

120014001600180020002200240026002800 scattering measurement with flashers scattering enhanced with dust logger data both scaled to position of hole 50

depth Μ m Ν b_e(400) Μ m^{-1} Ν

0 0.05 0.1 0.15 0.2 0.25 0.3 0.35 0.4

120014001600180020002200240026002800

AHA scattering coefficient b_e(400) merged dust logger and EDML data both scaled to position of hole 50

depth Μ m Ν b_e(400) Μ m^{-1} Ν

0 0.05 0.1 0.15 0.2 0.25 0.3 0.35 0.4

120014001600180020002200240026002800